P3：

01010011

+ 01100110

——————

10111001

+ 01110100

————————

00101110

Checksum:11010001

Checksum is used to detect errors.Receiver uses the checksum to add the original three bytes,if the sum has 0,then there is an error. The 1-bit error is impossible to be undetected,but the 2-bits errors will be undetected.

P8：

